****

**MEMORANDUM**

**DATE:        September 10, 2020**

**TO:             All Holders of Standard Plans**

**FROM:       Shawn Yu, Standards and Specifications Unit Manager**

**SUBJECT:  Revised Standard Plan - M-60​3-3 - Precast Concrete ​Box Culvert**

Effectively today, the Project Development Branch has issued the revised CDOT Standard Plan *M-603-3 - Precast Concrete Box Culvert​ ​*with ​1 sheet.

This revised standard plan replaces the ​July 31, 2020 version with the same name.

The revisions added a waterproofing membrane on top of Precast Concrete Box Culverts with fill heights less than 2 feet.  General Note 1 now includes LRFD design requirements per ASTM C 1577 for all precast concrete box culverts.  Added electronically sealed requirements in General Notes 1 and 2.

Use of this revised standard is required on all applicable projects advertised on or after October 12, 2020.  Earlier use of it is also permissible.

Please note that any new ​or revised M&S ​​Standards ​to be used in projects must have their corresponding ​box filled in ​the [Standard Plans List sheet](https://www.codot.gov/business/designsupport/2019-and-2012-m-standards/2019-m-standards-plans/2019-standard-plans-list) and inserted into the plan set.

Electronic copies of this and other standards are available on CDOT’s [2019 M Standard Plans and Project Special drawings](https://www.codot.gov/business/designsupport/2019-and-2012-m-standards/2019-m-standards-plans/2019-m-standards-plans-and-details) website.

If you have any questions or comments, please contact ​this office​.



2829 W. Howard Pl., 3rd floor, Denver, CO 80204 P 303.757.9474 F 303.757.9820 [www.codot.gov/](http://www.codot.gov/) |