July 1, 2010

REVISION OF SECTION 612

DELINEATORS

**NOTICE**

This is a standard special provision that revises or modifies CDOT’s *Standard Specifications for Road and Bridge Construction* It has gone through a formal review and approval process and has been issued by CDOT’s Project Development Branch with formal instructions for its use on CDOT construction projects. It is to be used as written without change. Do not use modified versions of this special provision on CDOT construction projects, and do not use this special provision on CDOT projects in a manner other than that specified in the instructions unless such use is first approved by CDOT’s Standards and Specifications Unit. The instructions for use on CDOT construction projects appear below.

Other agencies which use the *Standard Specifications for Road and Bridge Construction* to administer construction projects may use this special provision as appropriate and at their own risk.

**Instructions for use on CDOT construction projects:**

Use in projects having delineators.

July 1, 2010

REVISION OF SECTION 612

DELINEATORS

Section 612 of the Standard Specifications is hereby revised for this project as follows:

In subsection 612.02(a) 2.B, delete the first paragraph, and replace with the following:

B. Base Anchoring. The posts shall be designed to facilitate a permanent installation that resists overturning, twisting, and displacement from wind and impact forces. It shall have an anchoring depth of 18 to 24 inches. Actual depth shall be as recommended by the manufacturer, or as directed by the Engineer. If soil conditions prohibit anchoring depth to less than 18 inches, the anchor shall be embedded in concrete, as specified by the manufacturer and as directed by the Engineer.

In subsection 612.02(a) 2.E. delete (1) and replace with the following:

(1) Width. The post shall have a minimum width of 2-3/8 inches and a maximum width of 4-½ inches facing traffic.

Subsection 612.05 shall include the following:

Concrete for anchor embedment will not be measured and paid for separately, but shall be included in the work.