REVISION OF SECTION 203

EMBANKMENT MATERIAL

Section 203 of the Standard Specifications is hereby revised for this project as follows:

In subsection 203.03(a), first paragraph, after the second sentence add the following:

Embankment material shall have a ♦ value of at least ▲ when tested by the Hveem Stabilometer.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**INSTRUCTION TO DESIGNERS** (delete instruction and symbol from final draft):

♦ Insert either "resistance value" or "resilient modulus value", as appropriate.

▲ Insert the actual value. This value may be specified on the plans or in a plan note rather than using this special provision.