January 6, 2012

REVISION OF SECTION 109
MEASUREMENT OF WATER

**NOTICE**

This is a standard special provision that revises or modifies CDOT’s *Standard Specifications for Road and Bridge Construction.* It has gone through a formal review and approval process and has been issued by CDOT’s Project Development Branch with formal instructions for its use on CDOT construction projects. It is to be used as written without change. Do not use modified versions of this special provision on CDOT construction projects, and do not use this special provision on CDOT projects in a manner other than that specified in the instructions unless such use is first approved by CDOT’s Standards and Specifications Unit. The instructions for use on CDOT construction projects appear below.

Other agencies which use the *Standard Specifications for Road and Bridge Construction* to administer construction projects may use this special provision as appropriate and at their own risk.

**Instructions for use on CDOT construction projects:**

Use in all projects.

January 6, 2012

REVISION OF SECTION 109

MEASUREMENT OF WATER

Section 109 of the Standard Specifications is hereby revised for this project as follows:

In subsection 109.01, delete the twenty-sixth paragraph and replace with the following:

Water may be measured either by volume or weight. Water meters shall be accurate within a range of ± 3 percent. When water is metered, the Contractor shall use an approved metering device and shall furnish the Engineer a certificate showing the meter has been accurately calibrated within the time allowed in the following schedule:

|  |  |
| --- | --- |
| 2 inch | 4 years |
| 4 inch to 6 inch | 2 years |
| 8 inch to 10 inch | 1 year |