REVISION OF SECTION 624  
DRAINAGE PIPE

Section 624 of the Standard Specifications is hereby revised for this project as follows:

Subsection 624.02 shall include the following:

▲Reinforced concrete pipe shall be coated in accordance with subsection 706.07.

♦Aluminum and Aluminized Corrugated Steel pipe shall not be used.

**INSTRUCTIONS** **TO** **DESIGNERS** (delete instructions and symbols from final draft):

Consult the CDOT *Pipe Material Selection Policy* before using this worksheet to develop a special provision for inclusion in the Contract. If none of the following criteria apply to the Contract, a special provision based on this worksheet is not required.

▲ Use this statement when the specified class of pipe allows RCP and the pH of the soil or water is less than 5. See the CDOT *Pipe Material Selection Policy*.

♦ Use this statement even when the specified class of pipe allows Aluminum or Aluminized Corrugated Steel because if the abrasion level is higher than 1 it should not be used. See the CDOT Pipe Material Selection Policy.