

Standards and Specifications Unit

**Memorandum**

**DATE**: April 30, 2105

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Sections 105, 106, 412, 601 and 709, Conformity to the Contract of Portland Cement Concrete Pavement And Dowel Bars And Tie Bars For Joints

Effective this date, our unit is issuing a revised version of the standard special provision, Revision of Sections 105, 106, 412, 601 and 709, Conformity To The Contract Of Portland Cement Concrete Pavement And Dowel Bars And Tie Bars For Joints. This revised standard special provision is 24 pages long, and replaces the now outdated standard special provision dated January 15, 2015. The use of this revised Standard Special Provision is mandatory on projects having Concrete Class E and Class P, beginning with projects advertised on or after May 28, 2015.

The modifications in this revision change tining depth to texture depth and clarify the plan values for the incentive/disincentive calculation program.

Those of you who keep a book of Standard Special Provisions should replace the now obsolete standard special provision with this revised version. For your convenience, you can find this and others special provisions issued this date in one place at our Construction Specifications web page:

<https://www.codot.gov/business/designsupport/construction-specifications/2011-Specs>

Please scroll down and visit the hyperlink, “Recently Issued Special Provisions”.

If you have any questions or comments, please contact this office.