

Standards and Specifications Unit

**Memorandum**

**DATE**: February 23, 2017

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Sections 106, 627 and 713 Glass Beads for Pavement Marking

Effective this date, our unit is issuing a revised version of standard special provision, Revision of Sections 106, 627 and 713 Glass Beads for Pavement Marking. This revised standard special provision is 1 page long and replaces a standard special provision having the same title dated May 12, 2016.

Use this revised standard special provision in projects having pavement marking with glass beads, beginning with projects advertised on or after March 23, 2017. You are free to use this standard special provision in projects advertised before this date.

This revisions contained in this version increases the percent of the total weight of epoxy pavement marking that shall be manufactured using a molten kiln direct melt method. The new value is 50 percent, instead of 40 percent.

Those of you who keep a book of Standard Special Provisions should replace the now obsolete standard special provision with this revised version. For your convenience, you can find this and others special provisions issued this date in one place at our Construction Specifications web page:

 <https://www.codot.gov/business/designsupport/construction-specifications/2011-Specs>

Please scroll down and visit the hyperlink, “Recently Issued Special Provisions”.

If you have any questions or comments, please contact this office.