Sample project special: 401hmacswr

02-03-11

REVISION OF SECTION 401

HOT MIX ASPHALT COMPACTION

(STEEL WHEEL ROLLER)

Section 401of the Standard Specifications is hereby revised for this project as follows:

In subsection 401.17, first paragraph, delete the second sentence and replace with the following:

Steel wheel rollers will be required on this project.

**INSTRUCTIONS TO DESIGNERS AND REGION MATERIALS ENGINEERS** (delete instructions from final draft):

Use one of the two plant mix pavement compaction project special provisions on projects having Hot Mix Asphalt.

The designer should consult the Region Materials Engineer for guidance on roller requirements.

For specialty paving or proprietary products, the Region Materials Engineer may consult the manufacturer’s recommendations.

Use this project special provision to delete the pneumatic tire rollers on projects that have one or more of the following conditions:

- Stone Matrix Asphalt Mixes

- Highly Modified or Rubberized Polymer Binder Mixes

Pneumatic rollers should be required on projects that have one or more of the following conditions:

- Non-polymerized Binder Mixes

- Leveling Courses

- Hot In-Place Recycling

- Cold In-Place Recycling

Pneumatic tire rollers should be considered for the following projects only when Region experience has shown it to be appropriate:

- Polymerized Binder Mixes