Sample project special: 615rd

02-03-11

REVISION OF SECTION 615

ROCK DEFLECTOR

Section 615 of the Standard Specifications is hereby revised for this project as follows:

Subsection 615.01 shall include the following:

This work includes the placement of riprap to construct rock deflectors and channel lining in the proposed low flow channel.

Subsection 615.02 shall include the following:

Rock deflectors shall consist of native rock or stone meeting the requirements of subsection 506.02 and having typical stone dimensions of 12 to 18 inches.

Subsection 615.03 shall include the following:

The locations and configurations of rock deflectors shall be as shown on the plans, or as otherwise directed by the Engineer.

Subsection 615.04 shall include the following:

Rock deflectors will be measured by the actual number of installations placed.

Subsection 615.05 shall include the following:

**Pay Item Pay Unit**

Rock Deflector Each

Structure excavation and structure backfill for rock deflector will not be measured and paid for separately but shall be included in the work.