Sample project special: 210mm

02-03-11

REVISION OF SECTION 210

MODIFY MANHOLE

Section 210 of the Standard Specifications is hereby revised for this project as follows:

Subsection 210.01 shall include the following:

Modify manholes consists of raising existing sanitary sewer manholes to the new grade lines established with construction of roadway widening.

Subsection 210.02 shall include the following:

Modification of manholes shall be done in accordance with the details included in the plans and in conformance with the appropriate M Standard Plan.

Subsection 210.12 shall include the following:

Modify manholes will be measured by the actual number modified which shall include all work required to: remove portion of existing manholes to the top of the barrel, build new barrel to the required height, build new eccentric cones to the required height, add additional steps as required, and reset the manhole ring and cover to the finished grade. If the rings and covers are destroyed or in the opinion of the Engineer cannot be reused, new manhole rings and covers shall be provided.

Subsection 210.13 shall include the following:

Payment will be made under:

**Pay Item Pay Unit**

Modify Manhole Each

Structure excavation and structure backfill required for "Modify Manhole" will not be measured and paid for separately but shall be included in the work. Reinforcing steel, structural concrete, manhole rings and covers, as well as all other materials required to complete the item shall be included in the work.