January 30, 2014

REVISION OF SECTION 206

STRUCTURE BACKFILL AT BRIDGE ABUTMENTS

**NOTICE**

This is a standard special provision that revises or modifies CDOT’s *Standard Specifications for Road and Bridge Construction.* It has gone through a formal review and approval process and has been issued by CDOT’s Project Development Branch with formal instructions for its use on CDOT construction projects. It is to be used as written without change. Do not use modified versions of this special provision on CDOT construction projects, and do not use this special provision on CDOT projects in a manner other than that specified in the instructions unless such use is first approved by CDOT’s Standards and Specifications Unit. The instructions for use on CDOT construction projects appear below.

Other agencies which use the *Standard Specifications for Road and Bridge Construction* to administer construction projects may use this special provision as appropriate and at their own risk.

**Instructions for use on CDOT construction projects:**

Use in projects having bridge construction.

January 30, 2014

REVISION OF SECTION 206

STRUCTURE BACKFILL AT BRIDGE ABUTMENTS

Section 206 of the Standard Specifications is hereby revised for this project as follows:

In subsection 206.02 (a), delete the first sentence of the second paragraph and replace with the following:

Structure backfill (Class 1) with mechanical reinforcement shall be used to backfill bridge abutments, unless otherwise shown on the Plans. When structure backfill (flow-fill) is called for, it shall meet the following requirements.