May 5, 2011

REVISION OF SECTIONS 412, 601, AND 711
LIQUID MEMBRANE-FORMING COMPOUNDS
FOR CURING CONCRETE

**NOTICE**

This is a standard special provision that revises or modifies CDOT’s *Standard Specifications for Road and Bridge Construction*. It has gone through a formal review and approval process and has been issued by CDOT’s Project Development Branch with formal instructions for its use on CDOT construction projects. It is to be used as written without change. Do not use modified versions of this special provision on CDOT construction projects, and do not use this special provision on CDOT projects in a manner other than that specified in the instructions unless such use is first approved by CDOT’s Standards and Specifications Unit. The instructions for use on CDOT construction projects appear below.

Other agencies which use the *Standard Specifications for Road and Bridge Construction* to administer construction projects may use this special provision as appropriate and at their own risk.

**Instructions for use on CDOT construction projects:**

Use on projects having any type of concrete construction.

May 5, 2011

REVISION OF SECTIONS 412, 601 AND 711
LIQUID MEMBRANE-FORMING COMPOUNDS
FOR CURING CONCRETE

Sections 412, 601 and 711 of the Standard Specifications are hereby revised for this project as follows:

In subsection 412.14, first paragraph, delete the second sentence and replace with the following:

The impervious membrane curing compound shall meet the requirements of ASTM C 309, Type 2 and shall be volatile organic content (VOC) compliant.

In subsection 601.13 (b), first paragraph, delete the second sentence and replace with the following:

A volatile organic content (VOC) compliant curing compound conforming to ASTM C 309, Type 2 shall be used on surfaces where curing compound is allowed, except that Type 1 curing compound shall be used on exposed aggregate or colored concrete, or when directed by the Engineer.

In subsection 601.16 (a) 1., delete the first sentence and replace with the following:

1. Membrane Forming Curing Compound Method. A volatile organic content (VOC) compliant curing compound conforming to ASTM C 309, Type 2 shall be uniformly applied to the surface of the deck, curbs and sidewalks at the rate of 1 gallon per 100 square feet.

Delete subsection 711.01 and replace with the following:

**711.01 Curing Materials.** Curing materials shall conform to the following requirements:

|  |  |
| --- | --- |
| Burlap Cloth made from Jute or Kenaf | AASHTO M 182 |
| Liquid Membrane-Forming Compounds forCuring Concrete | ASTM C 309 |
| Sheet Materials for Curing Concrete | AASHTO M 171\* |
| \*Only the performance requirements of AASHTO M171 shall apply. |

Straw used for curing shall consist of threshed straw of oats, barley, wheat, or rye. Clean field or marsh hay may be substituted for straw when approved by the Engineer. Old dry straw or hay which breaks readily in the spreading process will not be accepted.