May 2, 2013

REVISION OF SECTIONS 401 AND 412

SAFETY EDGE

**NOTICE**

This is a standard special provision that revises or modifies CDOT’s *Standard Specifications for Road and Bridge Construction*. It has gone through a formal review and approval process and has been issued by CDOT’s Project Development Branch with formal instructions for its use on CDOT construction projects. It is to be used as written without change. Do not use modified versions of this special provision on CDOT construction projects, and do not use this special provision on CDOT projects in a manner other than that specified in the instructions unless such use is first approved by CDOT’s Standards and Specifications Unit. The instructions for use on CDOT construction projects appear below.

Other agencies which use the *Standard Specifications for Road and Bridge Construction* to administer construction projects may use this special provision as appropriate and at their own risk.

**Instructions for use on CDOT construction projects:**

Use on projects having any type of roadway pavement.

May 2, 2013

1

REVISION OF SECTIONS 401 AND 412

SAFETY EDGE

Sections 401 and 412 of the Standard Specifications are hereby revised for this project as follows:

Subsection 401.10 shall include the following:

The paver shall include an approved longitudinal paver wedge system to create a sloped safety edge as shown on the plans. The wedge system shall be attached to the screed and shall compact the HMA to a density at least as dense as the compaction imparted to the rest of the HMA layer by the paving screed. The system shall provide a sloped Safety Edge equal to 32 degrees plus or minus 5 degrees measured from the pavement surface cross slope extended. The use of a single plate strike off is not permitted. The system shall be adjustable to accommodate varying paving thicknesses. The Engineer may allow the Contractor to use handwork for short sections or to saw cut the sloped Safety Edge after paving operations are completed in areas such as transitions at driveways, intersections, interchanges.

The Contractor shall submit the proposed system for approval at the Preconstruction Conference. The Engineer may require proof that the system has been used on previous projects with acceptable results or may require a test section constructed prior to the beginning of work to demonstrate that it creates an acceptable wedge shape and compaction. Paving shall not begin until the system is approved in writing by the Engineer. The Safety Edge may be constructed on each lift of HMA or on the full specified plan depth on the final lift. The finished shape of the Safety Edge shall extend for the full depth of the asphalt pavement or for the top 5 inches whichever is less.

Subsection 401.22 shall include the following:

All costs associated with the construction of the Safety Edge will not be paid for separately, but shall be included in the work.

Subsection 412.07 shall include the following:

The Contractor shall use an approved longitudinal paver wedge system to create a sloped Safety Edge. The Contractor shall modify the paver screed to create a Safety Edge that meets the final cross-section shown on the plans. The system shall provide a sloped Safety Edge equal to 32 degrees plus or minus 5 degrees measured from the pavement surface cross slope extended. There may be areas where it is not possible to place the Safety Edge in conjunction with mainline paving but where the Safety Edge is required, such as transitions at driveways, intersections, interchanges, etc. In these areas the Engineer may allow the Contractor to use handwork for short sections or to saw cut the sloped Safety Edge after paving operations are completed.

The Contractor shall submit the proposed system for approval at the Preconstruction Conference. The Engineer may require proof that the system has been used on previous projects with acceptable results or may require a test section constructed prior to the beginning of work to demonstrate that it creates an acceptable wedge shape. Paving shall not begin until the system is approved in writing by the Engineer. The finished shape of the Safety Edge shall extend for the full depth of the concrete pavement or for the top 5 inches whichever is less.

May 2, 2013

2

REVISION OF SECTIONS 401 AND 412

SAFETY EDGE

Subsection 412.23 shall include the following:

Concrete Safety Edge will be measured by the actual number of linear feet that are installed and accepted.

Subsection 412.24 shall include the following:

Pay Item Pay Unit

Concrete Safety Edge Linear Foot

Payment for concrete safety edge will be full compensation for all work and materials required to complete the item.