REVISION OF SECTION 304

AGGREGATE BASE COURSE

Section 304 of the Standard Specifications is hereby revised for this project as follows:

Subsection 304.02 shall include the following:

Materials for the subbase shall be Aggregate Base Course (Class ♦) as shown in subsection 703.03.

Materials for the base course shall be Aggregate Base Course (Class**♦**) as shown in subsection 703.03

The aggregate base course (Class ▲) and (Class ▲) must meet the gradation requirements and have a resistance value of at least ♥ and ♥ respectively when tested by the Hveem Stabilometer method.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**INSTRUCTIONS TO DESIGNERS** (delete instructions and symbols from final draft):

**♦** Use when appropriate, inserting the proper Class of base course.

▲ Use for all Classes of base course, inserting the correct figures.

♥ Insert the specified resistance values.