**REVISION OF SECTION 210  
REPAIR CURB RAMPS AND SIDEWALK**

Section 210 of the Standard Specifications is hereby revised for this project as follows:

Subsection 210.02 shall include the following:

**Curb Ramp Repair:** The Contractor shall diamond grind areas where existing ramp joints between the roadway surface and gutter pan are not flush and where the ramp grade breaks are not flush. The Contractor shall grind joints and grade breaks that have an existing vertical displacement of 1/8 inch to 2 inches. The Contractor shall notify the Engineer of locations where the ramp contains a displacement greater than 2 inches before proceeding with repairs.

Completed grinds shall be smooth and sloped back at a rate of 7.5 percent or flatter. The final surface of the ground area shall be even and uniform in appearance.

Where necessary, the adjacent curb surface shall be ground to match.

Repair locations shall be as shown on the plans or as directed by the Engineer.

**Sidewalk and Multiuse Trail Repair:** Minor repairs for sidewalks and multiuse trails shall be made by diamond grinding. Vertical surface discontinuities between ¼ inch and ½ inch shall be beveled with a slope of 50 percent or flatter. The bevel shall be applied across the entire vertical surface discontinuity.

Repair locations shall be as shown on the plans or as directed by the Engineer.

**Sidewalk Slope Correction:** Correction of sidewalk slope shall be made by diamond grinding.

Repair locations shall be as shown on the plans or as directed by the Engineer.

Subsection 210.12 shall include the following:

Curb ramp repair will be measured by the linear foot of ramp-roadway joints and ramp grade breaks that are repaired by diamond grinding.

Sidewalk and multiuse trail repair will be measured by the linear foot of surface discontinuities that are repaired by diamond grinding.

Sidewalk slope correction will be measured by the actual number of square feet that are diamond ground.

Subsection 210.13 shall include the following:

Payment will be made under:

**Pay Item Pay Unit**

Grinding: Sidewalk and/or Curb Ramp Repair LF

Grinding: Slope Correction SF

Payment for diamond grinding will be full compensation for all work and materials necessary to complete the item.