Sample project special: 607rcg

02-03-11 (Re-issued 07-03-17)

REVISION OF SECTION 607

ROAD CLOSURE GATE

Section 607 of the Standard Specifications is hereby revised for this project as follows:

Subsection 607.01 shall include the following:

This work includes the fabrication and construction of a road closure gate in accordance with the plans.

Subsection 607.02 shall include the following:

Luminaire lamps shall be high pressure sodium and 250 watts.

Subsection 607.04 shall include the following:

Road closure gates will be measured by the actual number of gates that are installed and accepted.

Subsection 607.05 shall include the following:

# Pay Item Pay Unit

Road Closure Gate Each

Payment for road closure gates will be full compensation required for all labor, materials and equipment required to fabricate and install the gate, including drilled shaft foundation, light standard, luminaire, mast arm, gate assembly, direct burial cable, excavation, embankment, sand, conduit, wiring, and “Road Closed” sign.

Power connection for road closure gates will be paid for in accordance with subsection 109.04.