Revise Section 504 of the Standard Specifications for this project as follows:

Delete the first paragraph of Section 504.15 for this project and replace it with the following:

**504.15** **Verification Testing of Sacrificial Soil Nails.** The total number and location of tests shall be determined and spaced to evaluate soil nail performance in each soil unit encountered along the total length of the wall. A minimum of two verification tests shall be performed on sacrificial test soil nails at each soil nail wall as shown on the plans or as directed by the Engineer. Verification testing shall be performed prior to installation of production soil nails to confirm the appropriateness of the Contractor’s drilling and installation methods and verify the required soil nail pullout resistance. If the Contractor makes changes to the drilling or soil nail installation operation or variability in the soil conditions is encountered, the Engineer may request additional verification tests.