**Revise Section 518 of the Standard Specifications as follows:**

**Revise Subsection 518.05 (a) as shown:**

(a)  The ~~transverse separation beams (center beams), support bars, and other structural elements~~ center beam/support bar connection, field-splice, and other bolted and welded connection details in the joint shall be fatigue tested and designed following the guidelines provided in ~~NCHRP Report 402, “Fatigue Design of Modular Bridge  Expansion Joints”~~ Appendix A19 of the latest edition of the AASHTO LRFD Bridge Construction Specification as well as the provisions included in Chapter 14 of the latest edition of the AASHTO LRFD Design Specification.  The Contractor shall provide calculations electronically sealed by the Contractor’s Engineer to the Engineer.