**Revise Section 208 of the Standard Specifications for this project as follows:**

**Subsection 208.10(b) shall include the following:**

The permanent BMPs to be surveyed will be discussed at the Environmental Preconstruction Conference.

Listed below are the permanent water quality BMPs to be surveyed:

♦

**INSTRUCTIONS TO DESIGNERS** (Delete instructions and symbols from final draft.):

♦ Insert the permanent water quality BMPs to be surveyed including station locations and offset (examples are listed below):

Extended Detention Basin

Infiltration Facility

Permanent Water Quality Inlet/Vault

Permanent Water Quality Swale

Retention Pond

Permanent Water Quality Constructed Wetland

Porous Surface

If Surveying (Lump Sum) is already included as a pay item, make sure to include the Survey Tabulation Data Sheet in the plans and mark the Permanent Water Quality BMP item listed under “Minor Structures” in the 2nd column.

Use Survey (Hour) if there is little or no other survey work on the project. In this case add the 625 project special provision Revision of Section 625 Permanent Water Quality BMP As Constructed Survey shown below.

REVISION OF SECTION 625

PERMANENT WATER QUALITY BMP

AS CONSTRUCTED SURVEY

**Revise Section 625 of the Standard Specifications for this project as follows:**

**Subsection 625.12 shall include the following:**

**625.12** Construction surveying of permanent BMPS will be measured by the hour.

Subsection 625.13 shall include the following:

**Pay Item Pay Unit**

Surveying Hour

All work and materials required to perform the permanent BMP survey and furnish the three electronic files shall be included in the original unit price bid for surveying.