REVISION OF SECTION 603

REINFORCED CONCRETE PIPE

Section 603 of the Standard Specifications is hereby revised for this project as follows:

Subsection 603.02 shall include the following:

♦Reinforced concrete pipe shall be manufactured from concrete that meets the requirements for severity of sulfate exposure Class ♦ specified in subsection 601.04.

▲Reinforced concrete pipe shall be coated in accordance with subsection 706.07.

**INSTRUCTIONS** **TO** **DESIGNERS** (delete instructions and symbols from final draft):

Consult the CDOT *Pipe Material Selection Policy* before using this worksheet to develop a special provision for inclusion in the Contract. Use this worksheet ONLY when use of a single pipe material is justified in accordance with the CDOT *Pipe Material Selection Policy*. Otherwise, pay for the pipe using the Section 624 pay item of the appropriate class.

♦ Use this statement only when the Section 603 pay item reinforced concrete pipe is specified. Insert the appropriate sulfate exposure class determined in accordance with the CDOT *Pipe Material Selection Policy*.

▲ Use this statement only when the Section 603 pay item reinforced concrete pipe is specified and the pH of the soil or water is less than 5. See the CDOT *Pipe Material Selection Policy*.