Sample Project Special: 202ram

02-03-11 (Re-issued 07-03-17)

REVISION OF SECTION 202

REMOVAL OF ASPHALT MAT

Section 202 of the Standard Specifications is hereby revised for this project as follows:

Subsection 202.01 shall include the following:

This work includes removal and disposal of existing asphalt mat within the project limits as shown on the plans or at locations directed by the Engineer.

In subsection 202.02 delete the seventh paragraph and replace with the following:

The existing asphalt mat which varies in thickness from 2.5 inches to 6 inches shall be removed in a manner that minimizes contamination of the removed mat with underlying material. The removed mat shall become the property of the Contractor and shall be either disposed of outside the project site, or used in one one or more of the following ways:

1. Used in embankment construction in accordance with subsection 203.07(c).

2. Placed in bottom of fills as approved by the Engineer.

3. Recycled into the hot mix asphalt.

4. Placed in the subgrade soft spots as directed by the Engineer.

Subsection 202.11 shall include the following:

The removal of the existing asphalt mat will be measured by the square yard of mat removed to the required depth and accepted.

Subsection 202.12 shall include the following:

Payment will be made under:

**Pay Item Pay Unit**

Removal of Asphalt Mat Square Yard

Unless otherwise specified in the Contract, the disposal of the asphalt mat or its use in other locations on the project will not be measured and paid for separately, but shall be included in the work.