Sample project special: 213md

02-03-11 (Re-issued 07-03-17)

REVISION OF SECTION 213

MULCHING (DECORATIVE)

Section 213 of the Standard Specifications is hereby revised for this project as follows:

Subsection 213.01 shall include the following:

Mulching (decorative) consists of placing 1.5 inch river rock at a depth of 4 inches in areas indicated on the plans or as designated.

Subsection 213.02 shall include the following:

Mulching (Decorative) shall consist of 1.5 inch washed, rounded, gray‑toned river rock. A sample shall be submitted in advance to the Engineer for approval.

Subsection 213.03 shall include the following:

The Contractor shall excavate as necessary to install Mulching (Decorative) as follows:

Mulching (Decorative) shall be contained within existing curb by grading to a depth of 6 inches along back of curb and tying smoothly to existing grade.

Mulching (Decorative) shall be placed over weed barrier fabric to a uniform depth of 4 inches in areas indicated on the plans or as designated.

Subsection 213.04 shall include the following:

Mulching (Decorative) will be measured by the cubic foot placed in accordance with the foregoing requirements.

Subsection 213.05 shall include the following:

**Pay Pay Unit**

Mulching (Decorative) Cubic Foot

Excavation required to place Mulching (Decorative) will not be paid for separately but shall be included in the work.