**Revise Section 107 of the Standard Specifications as follows:**

**Revise Section 107.07 as follows:**

107.07 Performance of Safety Critical Work

(13) Caissons and/or directional boring in high density utility corridor.  This includes open holes for new drilled shafts within two shaft diameters of existing drilled shafts and structures.

**Revise Section 503.02 as follows:**

 503.02 Submittals

(b) 10. Details and procedures for protecting existing structures, utilities, roadway and other facilities during drilled shaft installation.  The stability of the existing structures is the responsibility of the contractor.  Any new drilled shaft that is placed next to existing structures/drilled shafts with the potential to affect stability shall be considered safety critical work and shall follow the submittal requirements as specified in subsection 107.07.