**Revision of Section 603**

**Reinforced Concrete Pipe**

# Revise Section 603 of the Standard Specifications for this project as follows:

**Subsection 603.02 shall include the following:**

♦Reinforced concrete pipe shall be manufactured from concrete that meets the requirements for severity of sulfate exposure Class ♦ specified in subsection 601.04.

▲Reinforced concrete pipe shall be coated per subsection 706.07.

**Instructions** **to** **Designers** (delete instructions and symbols from final draft):

Consult the CDOT *Pipe Material Selection Policy* before using this worksheet to develop a special provision for inclusion in the Contract. Use this worksheet ONLY when use of a single pipe material is justified per the CDOT *Pipe Material Selection Policy*. Otherwise, pay for the pipe using the Section 624 pay item of the appropriate class.

♦ Use this statement only when the Section 603 pay item reinforced concrete pipe is specified. Insert the appropriate sulfate exposure class determined per the CDOT *Pipe Material Selection Policy*.

▲ Use this statement only when the Section 603 pay item reinforced concrete pipe is specified, and the pH of the soil or water is less than 5. See the CDOT *Pipe Material Selection Policy*.