Sample project special: 610mcms

02-03-11 (Re-issued 07-03-17)

REVISION OF SECTION 610

MEDIAN COVER MATERIAL (STONE)

Section 610 of the Standard Specifications is hereby revised for this project as follows:

Subsection 610.02 shall include the following:

Stone for median cover shall be 4 to 8 inch rounded river rock cobble and gray toned in color. The Contractor shall submit a sample of stone to the Engineer for approval prior to delivery and placement.

Subsection 610.03(c) shall include the following:

Stone shall be placed in a manner that will not puncture plastic sheeting.