**Revision Of Section 401**

**SafetyEdge**SM **for Pavement**

**Notice**

The Standard Special Provision (SSP) on the following page revises or modifies CDOT’s*Standard Specifications for Road and Bridge Construction.* The Construction Engineering Services Branch has reviewed, approved, and issued it. Use as written without change. Do not use modified versions of it on CDOT construction projects. Do not use the following special provision on CDOT projects in a manner other than specified in the instructions without approval by CDOT’s Standards and Specifications Unit. The instructions for use appear below.

Other agencies using the *Standard Specifications for Road and Bridge Construction*to administer construction projects may use this special provision appropriately and at their own risk.

**Instructions for use on CDOT construction projects:**

Use the following standard special provision on all projects with concrete or asphalt paving.

**Revision Of Section 401**

**SafetyEdge**SM **for Pavement**

**Revise Section 401 of the Standard Specifications as follows:**

**Subsection 401.01 shall include the following, at the end of the second paragraph:**

This work consists of one or more courses of asphalt mixture constructed on a prepared foundation per these specifications and the specific requirements of the type under contract, and in conformity with the lines, grades, thicknesses, and typical cross sections shown on the plans or established, including a beveled SafetyEdgeSM.

**Subsection 401.02 shall include the following, before Table 401-2:**

HMA for safety edge treatment must comply with Section 403, Hot Mix Asphalt, of the Standard Specifications.

Materials used in constructing the SafetyEdgeSM shall match the adjacent roadway material requirements.

**In subsection 401.10, replace the third sentence within the fourth paragraph as shown below:**

The system shall provide a sloped SafetyEdgeSM as per M-400-1, SafetyEdgeSM for Pavement.

**In subsection 401.10, include the following after the fifth paragraph:**

Provide a SafetyEdgeSM as per M-400-1, SafetyEdgeSM for Pavement, or as shown on the plans.

**In subsection 401.21, add the following after the first sentence:**

Full compensation for constructing the SafetyEdgeSM treatments is included in the contract price for the type of HMA designated. Site preparation and/or grading required to receive the SafetyEdgeSM treatment shall be paid per M-400-1, Note 8.

Full compensation to furnish, place, and compact shoulder or embankment material to the top of the SafetyEdgeSM is included in the contract price for the type of shoulder backing material designated or as equipment hours.

Full-depth sawing to remove integrally placed SafetyEdgeSM where not required, or construction of formed “box-out” to prevent placement during paving, is incidental to the contract.

No additional compensation will be allowed.