# Revision of Section 608 Curb Ramp (Temporary)

**Revise Section 608 of the Standard Specifications for this project as follows:**

## Subsection 608.01 shall include the following:

This work consists of the construction of a temporary curb ramp which is fully ADA compliant with current PROWAG guidelines and CDOT Standard DS-630-2a when constructed in work zones at locations as shown on the plans and CDOT Standard DS-630-1a.

## Subsection 608.02 shall include the following:

The temporary curb ramp shall be made of an approved durable material coated with a slip-resistant surface. The width of the temporary curb ramp shall be a minimum of 48 inches, and when required, a landing shall be attached. The slope of the ramp shall be no more than 1V:12H. The temporary curb ramp shall accommodate a minimum weight of 800 pounds and have free draining surfaces.

Protective edging shall be installed on both sides of the temporary curb ramp when the drop is 3 inches or more. Edging shall be continuous and a minimum of 6 inches high.

The Contractor shall submit manufacturer’s documentation or details stamped by a professional engineer confirming that the temporary curb ramp meets all applicable ADA requirements.

## Subsection 608.03 shall include the following:

1. Curb Ramp (Temporary). Construction and installation of the temporary curb ramp shall be in accordance with the Plans or manufacturer recommendations.

The ramp shall be installed either perpendicular or parallel to the curb. When the ramp is installed parallel to the curb of the roadway, a 48-inch by 48-inch (60-inch by 60-inch is preferred) landing shall be constructed of the same material at the top of the ramp. A continuous handrail shall be installed on both sides of the ramp with a rise greater than 6 inches at a minimum height of 34 inches (38 inch maximum), extending through the landing.

The ramp may be moved to other locations as shown on the plans or as directed upon completion of use at one location.

## Subsection 608.05 shall include the following:

Curb Ramp (Temporary) will be measured as the actual number installed and accepted.

## Subsection 608.06 shall include the following:

Payment will be made under:

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| Curb Ramp (Temporary) (Perpendicular) | Each |
| Curb Ramp (Temporary) (Parallel) | Each |

Movement of the temporary curb ramp to different locations, when required, will not be measured and paid for separately, but shall be included in the work.