MEMORANDUM

**DEPARTMENT OF TRANSPORTATION**

Project Development Branch

4201 East Arkansas Avenue

Denver, Colorado 80222

(303)757-9040

FAX (303)757-9868



**DATE**: August 19, 2011

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Section 108, Critical Path Method

Effective this date, our unit is issuing a revised version of the standard special provision, Revision of Section 108, Critical Path Method. This revised standard special is 1 page long. It replaces a now obsolete standard special provision of same title dated May 5, 2011. This revised standard special should be used in all projects, beginning with projects advertised on or after September 1, 2011. Please feel free, however, to include it in projects advertised before this date.

The modifications contained in this revision correct an inadvertent erratum in the 2011 edition of the Standard Specifications. It reintroduces language from the 2005 edition which requires the Contractor to submit a bar chart or initial schedule at least 10 working days prior to start of work.

Those of you who keep books of Standard Special Provisions should replace the now obsolete version of this special provision with this revised one. For your convenience, we are attaching a new Index of Standard Special Provisions. In addition, you will find this and other special provisions that are being issued this date in one place in the CDOT Construction Specifications web site:

<http://www.coloradodot.info/business/designsupport/construction-specifications/2011-Specs>

Please click on the hyperlink titled “Specification Changes Under Consideration” to access this and other special provisions that have been issued as of this date.

LB/mrs

Attachments

Distribution: Per distribution list