January 31, 2013

REVISION OF SECTION 630

SIGNS AND BARRICADES

**NOTICE**

This is a standard special provision that revises or modifies CDOT’s *Standard Specifications for Road and Bridge Construction.* It has gone through a formal review and approval process and has been issued by CDOT’s Project Development Branch with formal instructions for its use on CDOT construction projects. It is to be used as written without change. Do not use modified versions of this special provision on CDOT construction projects, and do not use this special provision on CDOT projects in a manner other than that specified in the instructions unless such use is first approved by CDOT’s Standards and Specifications Unit. The instructions for use on CDOT construction projects appear below.

Other agencies which use the *Standard Specifications for Road and Bridge Construction* to administer construction projects may use this special provision as appropriate and at their own risk.

**Instructions for use on CDOT construction projects:**

Use in projects having construction signing.

January 31, 2013

REVISION OF SECTION 630

SIGNS AND BARRICADES

Section 630 of the Standard Specifications is hereby revised for this project as follows:

In subsection 630.02, delete the second paragraph, and replace with the following:

Temporary sign support assembly shall be timber, perforated square metal tubing inserted into a larger base post or slip base or perforated metal U-channel with a slip base. The temporary sign support assembly shall conform to NCHRP and AASHTO requirements regarding temporary sign supports during construction.

Subsection 630.02 shall include the following:

If a timber post is selected, it shall conform to the requirements of subsection 614.02.