January 30, 2014

REVISION OF SECTION 107

WARNING LIGHTS FOR WORK VEHICLES AND EQUIPMENT

**NOTICE**

This is a standard special provision that revises or modifies CDOT’s *Standard Specifications for Road and Bridge Construction*. It has gone through a formal review and approval process and has been issued by CDOT’s Project Development Branch with formal instructions for its use on CDOT construction projects. It is to be used as written without change. Do not use modified versions of this special provision on CDOT construction projects, and do not use this special provision on CDOT projects in a manner other than that specified in the instructions unless such use is first approved by CDOT’s Standards and Specifications Unit. The instructions for use on CDOT construction projects appear below.

Other agencies which use the *Standard Specifications for Road and Bridge Construction* to administer construction projects may use this special provision as appropriate and at their own risk.

**Instructions for use on CDOT construction projects:**

Use in all projects.

January 30, 2014

REVISION OF SECTION 107

WARNING LIGHTS FOR WORK VEHICLES AND EQUIPMENT

Section 107 of the Standard Specifications is hereby revised for this project as follows:

Subsection 107.06 (b) shall include the following:

All work vehicles and mobile equipment shall be equipped with one or more functioning warning lights mounted as high as practicable, which shall be capable of displaying in all directions one or more flashing, oscillating, or rotating lights for warning roadway traffic. The lights shall be amber in color. The warning lights shall be activated when the work vehicle or mobile equipment is operating within the roadway, right of way or both. All supplemental lights shall be SAE Class 1 certified.