

Standards and Specifications Unit

**Memorandum**

**DATE**: April 30, 2015

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Section 601, Entrained Air of Class BZ Concrete

Effective this date, our unit is issuing a new standard special provision, Revision of Section 601, Entrained Air. This standard special provision is 1 page long. It is to be used in projects having any type of concrete construction, beginning with projects advertised on or after May 28, 2015. You are free to use it in projects advertised before this date.

This new standard special provision requires air entrainment to be included in the mix design for Class BZ concrete.

Those of you who keep a book of Standard Special Provisions should add this new spec to your file. For your convenience, you can find this and others special provisions issued this date in one place at our Construction Specifications web page:

<https://www.codot.gov/business/designsupport/construction-specifications/2011-Specs>

Please scroll down and visit the hyperlink, “Recently Issued Special Provisions”.

If you have any questions or comments, please contact this office.