MEMORANDUM

**DEPARTMENT OF TRANSPORTATION**

Project Development Branch

4201 East Arkansas Avenue

Denver, Colorado 80222

(303)757-9040

FAX (303)757-9868



**DATE**: May 5, 2011

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Section 108, Critical Path Method

Effective this date, our unit is issuing a new standard special provision, Revision of Section 108, Critical Path Method. This new standard special is 1 page long. It should be used in all projects, beginning with projects advertised on or after June 2, 2011. Please feel free, however, to include it projects advertised before this date.

This new standard special provision clarifies CDOT will not provide salient features when the Critical Path Method is to be submitted by the Contractor. Salient features are only provided by CDOT when a bar chart method is allowed.

Those of you who keep books of Standard Special Provisions should add this standard special to your file. For your convenience, we are attaching a new Index of Standard Special Provisions, dated May 5, 2011. In addition, you will find this and other special provisions that are being issued this date in one place in the CDOT Construction Specifications web site:

<http://www.coloradodot.info/business/designsupport/construction-specifications/2011-Specs/recently-issued-special-provisions>

If you have any questions or comments, please contact this office.

LB/mrs

Attachments

Distribution: Per distribution list