

Standards and Specifications Unit

**Memorandum**

**DATE**: October 29, 2015

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Sections 106 and 412, Surface Texture of Portland Cement Concrete Pavement

Effective this date, our unit is issuing a revised version of the standard special provision, Revision of Sections 106 and 412, Surface Texture of Portland Cement Concrete Pavement. This revision is 3 pages long and replaces the now obsolete standard special provision of the same title dated April 30, 2015.

The use of this standard special provision is required on projects having any type of concrete pavement, beginning with projects advertised on or after November 26, 2015. You are free, however, to use it in projects advertised before this date.

The modifications in this revised special provision remove the option of "info" cylinder testing for opening pavements to traffic. The changes will require the use of maturity meters with cores as a backup.

Those of you who keep a book of Standard Special Provisions should replace the now obsolete version in your file with this revised version. For your convenience, you can find this and others special provisions issued this date in one place at our Construction Specifications web page:

 <https://www.codot.gov/business/designsupport/construction-specifications/2011-Specs>

Please scroll down and visit the hyperlink, “Recently Issued Special Provisions”.

If you have any questions or comments, please contact this office.