

Standards and Specifications Unit

**Memorandum**

**DATE**: May 25, 2017

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Section 504, Soil Nail Wall

Effective this date, our unit is issuing a revised version of the standard special provision, Revision of Section 504, Soil Nail Wall. This revised standard special provision is 12 pages long and replaces a special provision having the same title dated January 12, 2017.

Beginning immediately, use this revised standard special provision in projects having soil nail walls. A “revision under ad” is not required.

The changes contained in this revised version correct the method of measurement of the soil nail wall as being measured and paid for by the quantities for the five major components of the wall: soil nail, initial shotcrete facing, verification testing, excavation and underdrain. A description of how each item is to be measured and paid for is clarified.

Those of you who keep a book of Standard Special Provisions should replace the obsolete version of this standard special provision in your file with this revised version. For your convenience, you can find this and others special provisions issued this date in one place at our Construction Specifications web page:

<https://www.codot.gov/business/designsupport/2011-construction-specifications/2011-Specs>

Please scroll down and visit the hyperlink, “[Recently Issued Special Provisions](https://www.codot.gov/business/designsupport/2011-construction-specifications/2011-Specs/recently-issued-special-provisions)”.

If you have any questions or comments, please contact this office.