Sample project special: 506rs

02-03-11

REVISION OF SECTION 506

RIPRAP (SPECIAL)

Section 506 of the Standard Specifications is hereby revised for this project as follows:

Subsection 506.01 shall include the following:

Riprap (Special) consists of random placement of large boulders in the new stream channel.

Subsection 506.02 shall include the following:

Boulders shall consist of native rock or stone of approximate size depicted on the plans or as directed. Concrete or other artificial materials will not be permitted.

Subsection 506.03 shall include the following:

Boulders shall be randomly spaced singly or in clusters, as directed, to form a natural appearing channel configuration.

Subsection 506.04 shall include the following:

Riprap (Special) will be measured by the actual number of boulders placed.

Subsection 506.05 shall include the following:

Payment will be made under:

**Pay Item Pay Unit**

Riprap (Special) Each

Structure Excavation will not be paid for separately but shall be included in the work.