Sample project special: 621tb

02-03-11

SECTION 621

TEMPORARY BRIDGE

Section 621 is hereby added to the Standard Specifications for this project as follows:

**DESCRIPTION**

**621.01** This item includes loading, transporting, erecting, maintaining, removing, and returning the temporary bridge.

**MATERIALS**

**621.02** The temporary bridge is a Bailey Bridge in the possession of the Department. The Department will not charge a rental fee for the use of this bridge on this project.

**CONSTRUCTION REQUIREMENTS**

**621.03** The Contractor shall load and return the temporary bridge at the following site:

The Contractor shall make arrangements with Department maintenance personnel at least five days prior to the loading and returning dates.

The temporary bridge shall be erected at the location and in conformity with the lines and grades shown on the plans or established.

The Contractor shall be responsible for replacing any structural parts that are missing or damaged when the bridge is returned.

The Contractor shall band all components together before returning the bridge for storage.

The Contractor shall return the temporary bridge no later then 30 days after the new structure is opened to traffic.

**METHOD OF MEASUREMENT**

**621.04** Temporary Bridge will not be measured, but will be paid for on a lump sum basis.

**BASIS OF PAYMENT**

**621.05** The completed and accepted work for the temporary bridge will be paid for at the contract lump sum price. This price shall include all labor, equipment, and materials required to load, transport, erect, maintain, remove, and return the temporary bridge.

Payment will be made under:

**Pay Item Pay Unit**

Temporary Bridge Lump Sum