Sample project special: 206ebc

02-03-11

REVISION OF SECTION 206

EXCAVATION AND BACKFILL FOR CULVERTS

Section 206 of the Standard Specifications is hereby revised for this project as follows:

Subsection 206.07 shall include the following:

Structure excavation and structure backfill required for all culverts and extensions will not be measured and paid for separately but shall be included in the work.

**INSTRUCTIONS TO DESIGNERS** (delete instructions from final draft)

When using this special provision be sure to include in the plans a tabulation of structure excavation and backfill for information only, so Contractors can bid the project intelligently and so testers can schedule testing at the proper frequency.