July 19, 2012

REVISION OF SECTION 612

FLEXIBLE DELINEATORS

**NOTICE**

This is a standard special provision that revises or modifies CDOT’s *Standard Specifications for Road and Bridge Construction.* It has gone through a formal review and approval process and has been issued by CDOT’s Project Development Branch with formal instructions for its use on CDOT construction projects. It is to be used as written without change. Do not use modified versions of this special provision on CDOT construction projects, and do not use this special provision on CDOT projects in a manner other than that specified in the instructions unless such use is first approved by CDOT’s Standards and Specifications Unit. The instructions for use on CDOT construction projects appear below.

Other agencies which use the *Standard Specifications for Road and Bridge Construction* to administer construction projects may use this special provision as appropriate and at their own risk.

**Instructions for use on CDOT construction projects:**

Use in projects having flexible delineators.

July 19, 2012

REVISION OF SECTION 612

FLEXIBLE DELINEATORS

Section 612 of the Standard Specifications is hereby revised for this project to include the following:

Delete subsection 612.02 (a) 2, and replace with the following:

1. Flexible delineators shall be manufactured and supplied by:

Shur-Tite Products

PO Box 2283

Round Rock TX 78680

Contact: David Riker

512-218-9500 (office)

512-388-0417 (FAX)

512-971-0340 (Cell)

Ground-mounted delineator shall be Shur-Flex Driveable Delineator. Guardrail post mounted delineator shall be the Shur-Tite Guardrail Post Flat Mount Delineator or the Shur-Tite Guardrail Post Clamp Mount Delineator, as called for in the Contract. Surface mounted delineators shall be the Shur-Flex Surface Mount Delineators.

Subsection 612.03 shall include the following:

Flexible delineators shall be installed in accordance with manufacturer recommendations.

In subsection 612.03, delete the first sentence of the third paragraph and replace with the following:

The length of each reflector strip shall be as recommended by the manufacturer.

In subsection 612.04, delete the second sentence.

Subsection 612.05 shall include the following:

**Pay Item Pay Unit**

Delineator (Flexible) (Square Base) Each

Delineator (Flexible) (Flat Mounted) Each

Delineator (Flexible) (Clamp Mounted) Each

Delineator (Flexible) (Surface Mounted) Each

Payment will be full compensation for all work, materials, and equipment required to install the delineators.