February 18, 2016

REVISION OF SECTION 709

EPOXY COATED REINFORCING BARS

**NOTICE**

This is a standard special provision that revises or modifies CDOT’s *Standard Specifications for Road and Bridge Construction.* It has gone through a formal review and approval process and has been issued by CDOT’s Project Development Branch with formal instructions for its use on CDOT construction projects. It is to be used as written without change. Do not use modified versions of this special provision on CDOT construction projects, and do not use this special provision on CDOT projects in a manner other than that specified in the instructions unless such use is first approved by CDOT’s Standards and Specifications Unit. The instructions for use on CDOT construction projects appear below.

Other agencies which use the *Standard Specifications for Road and Bridge Construction* to administer construction projects may use this special provision as appropriate and at their own risk.

**Instructions for use on CDOT construction projects:**

Use in projects having any type of concrete construction.

February 18, 2016

REVISION OF SECTION 709

EPOXY COATED REINFORCING BARS

Section 709 of the Standard Specifications is hereby revised for this project as follows:

In subsection 709.01, delete the last row of the table and replace with the following

|  |  |
| --- | --- |
| Epoxy Coated Reinforcing Bars | AASHTO A 775 |

Delete the first sentence of subsection 709.03 and replace with the following:

Tie bars for longitudinal and transverse joints shall conform to AASHTO A 775 and shall be grade 40, epoxy-coated, and deformed.