

Standards and Specifications Unit

**Memorandum**

**DATE**: October 12, 2017

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Section 703, Classification for Aggregate Base Course

Effective this date, our unit is issuing a new standard special provision, Revision of Section 703, Classification for Aggregate Base Course. This new standard special provision is 1 page long.

Use this new standard special provision in projects having aggregate base course, beginning with projects advertised on or after November 9, 2017. You are free to use this standard special provision in projects advertised before this date.

This new standard special provision corrects minor errors in the 2017 Standard Specifications by providing a range of 95-100 percent for passing the 19 millimeters (3/4”) sieve for Class 6 aggregate. It also corrects the English units for 37.5 millimeters, changing the value from 2 inches to 1-1/2 inches.

Those of you who keep a book of Standard Special Provisions should add this new standard special provision to your file. For your convenience, you can find this and others special provisions issued this date in one place at our Construction Specifications web page:

<https://www.codot.gov/business/designsupport/cdot-construction-specifications/2017-construction-standard-specs/rev-ssp>

Please scroll down and visit the hyperlink, “[Recently Issued Special Provisions](https://www.codot.gov/business/designsupport/cdot-construction-specifications/2017-construction-standard-specs/recently-issued-special-provisions)”.

If you have any questions or comments, please contact this office.