NOTICE

This is a project special provision that revises or modifies CDOT’s *Standard Specifications for Road and Bridge Construction*. It has gone through a formal review and approval process and has been issued by CDOT’s Construction Engineering Services Branch with formal instructions for its use on CDOT construction projects. It is to be used as written without change. Do not use modified versions of this special provision on CDOT construction projects, and do not use this special provision on CDOT projects in a manner other than that specified in the instructions unless such use is first approved by CDOT’s Standards and Specifications Unit. The instructions for use on CDOT construction projects appear below.

Other agencies which use the *Standard Specifications for Road and Bridge Construction* to administer construction projects may use this special provision as appropriate and at their own risk.

**Instructions for use on CDOT construction projects:**

Use this standard special provision on all projects.

Section 105 of the Standard Specifications is hereby revised as follows:

Subsection 105.02 (f) shall include the following:

The Contractor shall provide pile and caisson tip elevations and provide all refusal & restrike information, driving records and PDA information to the Engineer prior to proceeding with further construction for permanent archiving.