Section 625 of the Standard Specifications is hereby revised for this project as follows:

###### Subsection 625.01 shall include the following:

Adobe Sign software shall be used for electronic seals by the Contractor’s Engineer, a Professional Engineer, or a Professional Land Surveyor. Electronic signatures and seals shall comply with the requirements of the Bylaws and Rules of the State Board of Licensure for Architects, Professional Engineers, and Professional Land Surveyors Rules and Regulations, 4 CCR 730-1.

######

###### Subsection 625.11, in the 2nd and 3rd paragraphs revise with the following:

All survey records generated shall be the property of the Department and shall be available to the Engineer for inspection or reproduction at all times. All survey records shall be transmitted to the Engineer for inclusion into the project records before final project acceptance. All survey records shall be electronically sealed by the responsible PLS or PE identified in subsection 625.01.

###### The electronically sealed survey records shall contain the same information and format as required in the Survey Manual Chapter 6, Section 6.1.15, including the stakeout data and the raw data from the actual placement of stakes and shall be submitted to the Engineer.

###### Subsection 625.13, in the 4th paragraph, revise with the following:

Before final payment is made, the following two items shall be completed and electronically sealed by the responsible PLS or PE identified in subsection 625.01, and have copies submitted to the Engineer for review:

1. All survey records.
2. Supplemental or amended Project Control Diagram (a copy of which shall be submitted to the Region Survey Coordinator).