Section 629 of the Standard Specifications is hereby revised for this project.

In Subsection 629.03 revise the fifth and sixth paragraphs with the following:

All survey records generated shall be the property of the Department and shall be available to the Engineer for inspection or reproduction at all times. All survey records shall be transmitted to the Engineer for inclusion into the project records before final project acceptance. All survey records shall be electronically sealed by the responsible PLS identified in subsection 629.01.

The electronically sealed survey records shall contain the same information and format as required in the Survey Manual Chapter 6, Section 6.1.15,including the stakeout data and the raw data from the actual placement of the monuments and shall be submitted to the Engineer.

In Subsection 629.05, last (4) revise with the following:

1. A n electronically sealed statement by the responsible PLS that states the replacement monument's positional tolerance has not been degraded. The documentation shall conform to the owner of the monument's specifications which control the work.

In Subsection 629.09 revise the third and fourth paragraphs with the following:

Legible electronically sealed copies of survey records in accordance with subsection 629.03 shall be submitted on a monthly basis to the Engineer for completed work before payment is made for that pay item.

Before final payment is made, the following three items shall be completed, be electronically sealed by the responsible PLS identified in subsection 629.01, and be submitted to the Engineer for review prior to being deposited with the county in accordance with Title 38 CRS, Property – Real and Personal, State Board Rules and Policies, MOU, and the CDOT Survey Manual:

1. All survey records.
2. The ROW Plans.
3. The Project Control Diagram (new, supplemental or amended).