REVISION OF SECTION 607  
TEMPORARY LIVESTOCK FENCE

Section 607 of the Standard Specifications is hereby revised for this project as follows:

Subsection 607.03 shall include the following:

All materials and debris generated from clearing and grubbing operations shall be removed from the project or otherwise properly disposed of in accordance with Section 201 Clearing and Grubbing.

1. *Temporary Livestock Fence*. Livestock may be pastured in various fields adjacent to the project during the construction of this project. In order to protect and control livestock, the Contractor shall install and maintain temporary fence of a type and at locations approved by the Engineer as needed during Construction. The Contractor shall maintain the temporary fence in such condition that it is capable of performing its intended function until such time as the permanent fence is completed. The Contractor shall give the landowner 30 days written notice before any existing fence or gates are removed.

Subsection 607.04 shall include the following:

Temporary Livestock Fence will not be measured and paid for separately, but shall be included in the work.