Sample project special: 207t

02-03-11 (Re-issued 07-03-17)

REVISION OF SECTION 207

TOPSOIL

Section 207 of the Standard Specifications is hereby revised for this project as follows:

Delete subsection 207.04 and replace with the following:

Topsoil material secured from the roadway and placed in stockpiles will be measured in the stockpile by the method of average end areas. This topsoil material will be paid for as Topsoil when placed on the slopes.

Topsoil secured from a source outside the right‑of‑way will be measured at its source as described in Section 203 and paid for as Topsoil.

In subsection 207.05 delete the Pay Item "Stockpile Topsoil."