# MARCH 18, 2021

# REVISION OF SECTION 710

# FENCE AND GUARDRAIL

Revise Section 710 of the Standard Specifications as follows:

Subsection 710.07 Fence Posts, revise the fourth paragraph to include:

Steel posts shall be galvanized in accordance with AASHTO M 111. Fittings, hardware and other appurtenances not specifically covered by the Contract shall be standard commercial grade, and in accord with current standard practice. Pipeor roll-formed steel material for fence posts shall conform to the requirements shown on the plans and to the requirements of Class 1 Pipe, Grade A and Grade B or Class 3 Formed Steel Sections, of Federal Specification RR-F-191/3E.