Section 62

Revise Section 625 of the Standard Specifications as follows:

Add subsection 625.04 (6) as follows:

1. The Contractor shall conduct an as-constructed survey of the following items: Installed or relocated utility lines as shown on the utility plans, including those installed or relocated by the Contractor or by others.
2. Installed or relocated culverts, conduit, inlets, or other drainage features.
3. Traffic signal heads, poles, pushbutton assemblies, and controller cabinets.
4. ITS fiber vaults, splice points, interfaces, nodes and other assets.
5. Lighting including pull boxes, meters and light standards.

The as-constructed survey shall be completed in accordance with the *CDOT Survey Manual*, Chapter 6, Section 6.14.