

**Memorandum**

**Date**: June 11, 2025

**To**: All holders of Standard Special Provisions

**From**: Bill Cornelius, Standards and Specifications Unit Manager

**Subject**: New standard special provision: Revision of Sections 412 and 601 – Accelerated

Pavement Repair Concrete

As of June 11, 2025, this unit has issued the new standard special provision, Revision of Sections 412 and 601 – Accelerated Pavement Repair Concrete, with 5 pages, and dated June 11, 2025.

This provision is to be used when project constraints limit lane closure time to 8 hours or less or when concrete needs to achieve opening strength of 2,500 psi in 6 hours or less, Class PRS concrete should be specified in the plan. Consult with the Region Materials Engineer before including Class PRS.

Please use this on all projects with Concrete Pavement Repair or Rehabilitation Activities.

This standard special provision will become mandatory in projects advertised on or after July 1, 2025. You may use this standard special provision in projects advertised before this date.

For those of you who keep a book of Standard Special Provisions, please include this new provision. For your convenience, this provision and the latest SSP Index are attached in the email. You can also find these in our Construction Specifications web pages: [Standard Special Provisions](https://www.codot.gov/business/designsupport/cdot-construction-specifications/2023-construction-specifications/rev-ssp/rev-sec100-ssp) and the [Recently Issued Special Provisions](https://www.codot.gov/business/designsupport/cdot-construction-specifications/2023-construction-specifications/recently-issued-special-provisions).

If you have any questions or comments, please contact this office.



 2829 W. Howard Pl., 3rd Fl. Denver, CO 80204 P: (720) 766-0420 F: 303-757-9868 [www.codot.gov](https://www.codot.gov/)