**REVISION OF SECTION OF 614**

**TRAFFIC SIGNAL FACES**

**Section 614 of the Standard Specification is hereby revised for this project as follows:**

**Subsection 614.08 (h) shall include the following:**

“Light Emitting Diode” (LED) signal lenses shall be installed in all Red, Yellow, Green, Walk and Don’t Walk, and Countdown signal displays. This work shall be included in the cost of the item for Traffic Signal Face and will not be paid for separately.